(footprint "Heatsink 60mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -1.27) (layer "F.SilkS"))
  (fp_text value "Heatsink 60mm" (at 0 1.27) (layer "F.Fab"))
  (pad "" np_thru_hole oval (at -25.5 -25.5) (size 4 4) (drill 3.1) (layers "F&B.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at -25.5 25.5) (size 4 4) (drill 3.1) (layers "F&B.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 25.5 -25.5) (size 4 4) (drill 3.1) (layers "F&B.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 25.5 25.5) (size 4 4) (drill 3.1) (layers "F&B.Cu" "*.Mask"))
)
