(footprint "SFD-0100-222" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -9.12 unlocked) (layer "F.SilkS"))
  (fp_text value "SFD-0100-222" (at 0 -7.62 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 -6.12 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole circle (at 1.27 -2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 1.27 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at 1.27 2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole circle (at -1.27 2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole circle (at -1.27 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole circle (at -1.27 -2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
)
